## **Firmware Update for Certain Pioneer In-Dash AV Receivers**

June 30, 2025

Dear Valued Pioneer Customer:

We would like to inform you of the availability of a firmware update for **only the following Pioneer** **In-Dash AV Receivers sold in** **the Middle East and Africa. Installation on any other product could cause irreversible damage.**

|  |
| --- |
| **DMH-AP6650BT** |

This firmware update corrects the following matter.

* Minor bug fix.

To perform this update, the following items are needed:

* Pioneer In-Dash AV Receiver
* Blank USB storage device (no files), 2 GB or larger in capacity, **must be formatted to** **FAT32**.

Instructions on installing the firmware are provided on the same page as the firmware update. Installation of the update should take about two minutes to complete.

**How to Obtain the Free Firmware Update:**

1. Download the firmware update files to a computer from the Pioneer website:

<https://pioneer-mea.com/en/software-and-firmware/>

1. Transfer the files to the USB storage device for insertion into the Pioneer In-Dash AV Receiver.

**Questions**

If you have any questions, please contact your nearest Pioneer Service Centre in your country:

<https://pioneer-mea.com/en/service-centres/>

Sincerely,

**Pioneer Gulf FZE**